TELEFUNKEN LED
Model: TF-LED50S7T2

Chassis/Version: CV9202H-T

Panel: CX500DLEDM

LED backlight: V500H1-ME1-TLEM9 LED 4020

LED driver (backlight): integrated into PSU

PWM LED driver: BIT3260

MOSFET LED driver: AOB254

Power Supply (PSU): CVB42001

PWM Power: LD7535 (PWM SOT23-6)

MOSFET Power: SMK1060

MainBoard: CV9202H-T

IC MainBoard: CPU: SPV9202BD(1416-D), DRAM :K4B1G1646G-BCKO, SPI FLASH :Winb25Q64FVSIG, AUDIO :TPA3110LD2

?uner: ST03WS-2A-E



















