ROLSEN RL-26X20

Panel: LC260WX2

T-CON: 12v

Inverter (backlight): KLS-EE26CI-M/S(P)

Trans Inverter: IT-094 0663

Power Supply (PSU): DMSM-S0007D

PWM Power: VIPER22A (Standby), L6562D (PFC), L6598D (PWM Resonant 16pin)

MOSFET Power: P11NM60 , W20NM60

MainBoard: DML-4126

IC MainBoard: CPU: SDA5550, EEPROM 24C16, flash A29040BL-70

Ňuner: TECH294PG40B(D)

Control: LC03-AR028A